# Wired Connection

1. Press the Stop button (A).

2. Select Wired LAN and press the OK button.

3. Select Yes and press the OK button.

4. You will need an Ethernet cable (sold separately).

5. Remove the Cap (B) from the port located on the left side at the back of the printer.

6. Connect the printer and a network device (router, etc.) with an Ethernet cable (C).

   Do not connect to any other port.

7. Press the OK button.

8. Press the OK button.

9. Return to the application software and proceed with the installation.

   Click in the taskbar, follow the on-screen instructions to proceed with setup.