# Wired Connection

1. Press the Setup button (A).

2. You will need an Ethernet cable (sold separately).

3. Remove the Cap (B) from the port located on the left side at the back of the printer.

4. Connect the printer and a network device (router, etc.) with an Ethernet cable (C).

   Do not connect to any other port.

5. Use the or button (D) to select Device settings and press the OK button.

6. Select LAN settings and press the OK button.

7. Select Wired LAN and press the OK button.

8. Select Enab./dis. wired LAN and press the OK button.

9. Select Enable and press the OK button.

10. If the screen on the below appears, press the OK button.

    If the following screen is not displayed, proceed to the next step.

11. Press the COPY button (E).

    The network connection setup is now complete.

12. Return to the application software and proceed with the installation.

    Click in the taskbar, follow the on-screen instructions to proceed with setup.