# Setup Guide
- G6000 series -

# Wired Connection

Follow the procedure below to setup a printer.

1. Make sure printer is turned on before starting wired connection setup.

   If the power is on, the ON lamp (A) will be lit or flashing.

   - Notes on Wired Connection(Appears in a new window)

   Important

   - If printer is performing cleaning, print head alignment, or other processes, wait for the process to finish, before starting setup.

2. Select the screen that is displayed on the printer's screen.

- When the screen on the left appears, see here

- When the screen on the left appears, see here

- If a different screen appears, see here