# The Select Network (SSID) Screen

If a connection between the printer and wireless router cannot be created automatically, the Select Network (SSID) screen is displayed.

Following the steps below, connect the printer and wireless router.

1. Select the network name (SSID) of the wireless router to which you want to connect from the Network Name (SSID): list.

   If your wireless router is not displayed in the list then follow the instructions in Wireless Router Not Available in Network Name (SSID) List.

2. Click Next.

   If you don't use encryption type, the following steps are not required.

3. Enter your wireless router's password in the Password: field.

   Enter the character you want to enter. Character entry is case-sensitive.

   If you are using a WEP connection, also set the WEP Key ID:.

4. Click Next.

## Wireless Router Not Available in Network Name (SSID) List

If your wireless router is not available in the Network Name (SSID): list, for example when stealth mode is set, following the steps below to add your wireless router.

1. Select the Other networks from the Network Name (SSID): list.

2. Click Next.

3. Enter network name (SSID) in the Network Name (SSID): field.

4. Select protocol from Encryption Type:.

   If you don't use encryption type, select Do not use and proceed to step 6.

   If you are using a WEP connection, also set the WEP Key Length:, WEP Key Format: and WEP Key ID:.

5. Enter your wireless router's password.

6. Click Next.

Note

- Password may be referred to as a Security Key or Passphrase.
- For information on the default values for you network name (SSID) and password, or how to check the currently set values, refer to the manual that came with your wireless router.
- SSIDs for the 2.4 GHz band appear for the network name (SSID). If your printer supports the 5 GHz band, SSIDs for the 5 GHz band also appear.