# Troubleshooting -WEP-

# "Failed to connect" Appears

1. Check1 Check the wireless router's settings.

   If the wireless router's DHCP function is off, turn it on or specify the printer's IP address (IPv4 only), and then redo the wireless connection settings. Also, make sure the selected WEP key number and entered password are correct.

## When specifying the IP address of the printer

Specify the printer's IP address as follows.

1. Press the Setup button.
2. Use the or button to select Device settings and press the OK button.
3. Select LAN settings and press the OK button.
4. Select Wi-Fi and press the OK button.
5. Select Manual setup and press the OK button.
6. Select TCP/IP settings and press the OK button.
7. Select IPv4 and press the OK button.
8. Press the OK button.
9. Select IP address and press the OK button.
10. Select Manual setup and press the OK button.

Follow the on-screen instructions to proceed with setup.

When setting is complete, press the Setup button and then redo the wireless connection.

- Enter the wireless router name directly again

1. Check2 When the DHCP function is active, enter wireless connection settings of the wireless router directly.

   - Enter the wireless router name directly again

2. Check3 When there is no problem with the WEP key number and password, enter the wireless router name directly.

   - Enter the wireless router name directly again

   For details on checking or changing the wireless router settings, see the wireless router manual or contact its manufacturer.